#
# Copyright (c) 2001-2003
#	Fraunhofer Institute for Open Communication Systems (FhG Fokus).
#	All rights reserved.
#
# Author: Harti Brandt <harti@bsdsunix.org>
#
# Redistribution and use in source and binary forms, with or without
# modification, are permitted provided that the following conditions
# are met:
# 1. Redistributions of source code must retain the above copyright
#    notice, this list of conditions and the following disclaimer.
# 2. Redistributions in binary form must reproduce the above copyright
#    notice, this list of conditions and the following disclaimer in the
#    documentation and/or other materials provided with the distribution.
#
# THIS SOFTWARE IS PROVIDED BY AUTHOR AND CONTRIBUTORS ``AS IS'' AND
# ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
# IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
# ARE DISCLAIMED.  IN NO EVENT SHALL AUTHOR OR CONTRIBUTORS BE LIABLE
# FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL
# DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS
# OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION)
# HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT
# LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY
# OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF
# SUCH DAMAGE.
#
# $Begemot: bsnmp/snmp_mibII/mibII_tree.def,v 1.13 2006/02/14 09:04:19 brandt_h Exp $
#
# Definition of the standard interfaces and ip trees.
#
(1 internet
  (2 mgmt
    (1 mib2
      (2 interfaces
        (1 ifNumber INTEGER op_interfaces GET)
        (2 ifTable
          (1 ifEntry : INTEGER op_ifentry
            (1 ifIndex INTEGER GET)
            (2 ifDescr OCTETSTRING GET)
            (3 ifType INTEGER GET)
            (4 ifMtu INTEGER32 GET)
            (5 ifSpeed GAUGE GET)
            (6 ifPhysAddress OCTETSTRING GET)
            (7 ifAdminStatus INTEGER GET SET)
            (8 ifOperStatus INTEGER GET)
            (9 ifLastChange TIMETICKS GET)
            (10 ifInOctets COUNTER GET)
            (11 ifInUcastPkts COUNTER GET)
            (12 ifInNUcastPkts COUNTER GET)
            (13 ifInDiscards COUNTER GET)
            (14 ifInErrors COUNTER GET)
            (15 ifInUnknownProtos COUNTER GET)
            (16 ifOutOctets COUNTER GET)
            (17 ifOutUcastPkts COUNTER GET)
            (18 ifOutNUcastPkts COUNTER GET)
            (19 ifOutDiscards COUNTER GET)
            (20 ifOutErrors COUNTER GET)
            (21 ifOutQLen GAUGE GET)
            (22 ifSpecific OID GET)
        ))
      )
      (4 ip
        (1 ipForwarding INTEGER op_ip GET SET)
        (2 ipDefaultTTL INTEGER op_ip GET SET)
        (3 ipInReceives COUNTER op_ipstat GET)
        (4 ipInHdrErrors COUNTER op_ipstat GET)
        (5 ipInAddrErrors COUNTER op_ipstat GET)
        (6 ipForwDatagrams COUNTER op_ipstat GET)
        (7 ipInUnknownProtos COUNTER op_ipstat GET)
        (8 ipInDiscards COUNTER op_ipstat GET)
        (9 ipInDelivers COUNTER op_ipstat GET)
        (10 ipOutRequests COUNTER op_ipstat GET)
        (11 ipOutDiscards COUNTER op_ipstat GET)
        (12 ipOutNoRoutes COUNTER op_ipstat GET)
        (13 ipReasmTimeout INTEGER32 op_ipstat GET)
        (14 ipReasmReqds COUNTER op_ipstat GET)
        (15 ipReasmOKs COUNTER op_ipstat GET)
        (16 ipReasmFails COUNTER op_ipstat GET)
        (17 ipFragOKs COUNTER op_ipstat GET)
        (18 ipFragFails COUNTER op_ipstat GET)
        (19 ipFragCreates COUNTER op_ipstat GET)
        (20 ipAddrTable
          (1 ipAddrEntry : IPADDRESS op_ipaddr
            (1 ipAdEntAddr IPADDRESS GET)
            (2 ipAdEntIfIndex INTEGER GET SET)
            (3 ipAdEntNetMask IPADDRESS GET SET)
            (4 ipAdEntBcastAddr INTEGER GET SET)
            (5 ipAdEntReasmMaxSize INTEGER GET)
        ))
        (22 ipNetToMediaTable
          (1 ipNetToMediaEntry : INTEGER IPADDRESS op_nettomedia
            (1 ipNetToMediaIfIndex INTEGER GET)
            (2 ipNetToMediaPhysAddress OCTETSTRING GET)
            (3 ipNetToMediaNetAddress IPADDRESS GET)
            (4 ipNetToMediaType INTEGER GET)
        ))
        (23 ipRoutingDiscards INTEGER op_ipstat)	# not available
        (24 ipForward
          (3 ipCidrRouteNumber GAUGE op_route GET)
          (4 ipCidrRouteTable
            (1 ipCidrRouteEntry : IPADDRESS IPADDRESS INTEGER IPADDRESS op_route_table
              (1 ipCidrRouteDest IPADDRESS GET)
              (2 ipCidrRouteMask IPADDRESS GET)
              (3 ipCidrRouteTos INTEGER GET)
              (4 ipCidrRouteNextHop IPADDRESS GET)
              (5 ipCidrRouteIfIndex INTEGER GET)	# SET
              (6 ipCidrRouteType INTEGER GET)		# SET
              (7 ipCidrRouteProto INTEGER GET)
              (8 ipCidrRouteAge INTEGER GET)
              (9 ipCidrRouteInfo OID GET)		# SET
              (10 ipCidrRouteNextHopAS INTEGER GET)	# SET
              (11 ipCidrRouteMetric1 INTEGER GET)	# SET
              (12 ipCidrRouteMetric2 INTEGER GET)	# SET
              (13 ipCidrRouteMetric3 INTEGER GET)	# SET
              (14 ipCidrRouteMetric4 INTEGER GET)	# SET
              (15 ipCidrRouteMetric5 INTEGER GET)	# SET
              (16 ipCidrRouteStatus INTEGER GET)	# SET
          ))
        )
      )
      (5 icmp
        (1 icmpInMsgs COUNTER op_icmpstat GET)
        (2 icmpInErrors COUNTER op_icmpstat GET)
        (3 icmpInDestUnreachs COUNTER op_icmpstat GET)
        (4 icmpInTimeExcds COUNTER op_icmpstat GET)
        (5 icmpInParmProbs COUNTER op_icmpstat GET)
        (6 icmpInSrcQuenchs COUNTER op_icmpstat GET)
        (7 icmpInRedirects COUNTER op_icmpstat GET)
        (8 icmpInEchos COUNTER op_icmpstat GET)
        (9 icmpInEchoReps COUNTER op_icmpstat GET)
        (10 icmpInTimestamps COUNTER op_icmpstat GET)
        (11 icmpInTimestampReps COUNTER op_icmpstat GET)
        (12 icmpInAddrMasks COUNTER op_icmpstat GET)
        (13 icmpInAddrMaskReps COUNTER op_icmpstat GET)
        (14 icmpOutMsgs COUNTER op_icmpstat GET)
        (15 icmpOutErrors COUNTER op_icmpstat GET)
        (16 icmpOutDestUnreachs COUNTER op_icmpstat GET)
        (17 icmpOutTimeExcds COUNTER op_icmpstat GET)
        (18 icmpOutParmProbs COUNTER op_icmpstat GET)
        (19 icmpOutSrcQuenchs COUNTER op_icmpstat GET)
        (20 icmpOutRedirects COUNTER op_icmpstat GET)
        (21 icmpOutEchos COUNTER op_icmpstat GET)
        (22 icmpOutEchoReps COUNTER op_icmpstat GET)
        (23 icmpOutTimestamps COUNTER op_icmpstat GET)
        (24 icmpOutTimestampReps COUNTER op_icmpstat GET)
        (25 icmpOutAddrMasks COUNTER op_icmpstat GET)
        (26 icmpOutAddrMaskReps COUNTER op_icmpstat GET)
      )
      (6 tcp
        (1 tcpRtoAlgorithm INTEGER op_tcp GET)
        (2 tcpRtoMin INTEGER32 op_tcp GET)
        (3 tcpRtoMax INTEGER32 op_tcp GET)
        (4 tcpMaxConn INTEGER32 op_tcp GET)
        (5 tcpActiveOpens COUNTER op_tcp GET)
        (6 tcpPassiveOpens COUNTER op_tcp GET)
        (7 tcpAttemptFails COUNTER op_tcp GET)
        (8 tcpEstabResets COUNTER op_tcp GET)
        (9 tcpCurrEstab GAUGE op_tcp GET)
        (10 tcpInSegs COUNTER op_tcp GET)
        (11 tcpOutSegs COUNTER op_tcp GET)
        (12 tcpRetransSegs COUNTER op_tcp GET)
        (13 tcpConnTable
          (1 tcpConnEntry : IPADDRESS INTEGER IPADDRESS INTEGER op_tcpconn
            (1 tcpConnState INTEGER GET)
            (2 tcpConnLocalAddress IPADDRESS GET)
            (3 tcpConnLocalPort INTEGER GET)
            (4 tcpConnRemAddress IPADDRESS GET)
            (5 tcpConnRemPort INTEGER GET)
        ))
        (14 tcpInErrs COUNTER op_tcp GET)
        (15 tcpOutRsts COUNTER op_tcp)		# don't know
      )
      (7 udp
        (1 udpInDatagrams COUNTER op_udp GET)
        (2 udpNoPorts COUNTER op_udp GET)
        (3 udpInErrors COUNTER op_udp GET)
        (4 udpOutDatagrams COUNTER op_udp GET)
        (5 udpTable
          (1 udpEntry : IPADDRESS INTEGER op_udptable
            (1 udpLocalAddress IPADDRESS GET)
            (2 udpLocalPort INTEGER GET)
        ))
      )
      (31 ifMIB
        (1 ifMIBObjects
          (1 ifXTable
            (1 ifXEntry : INTEGER op_ifxtable
              (1 ifName OCTETSTRING GET)
              (2 ifInMulticastPkts COUNTER GET)
              (3 ifInBroadcastPkts COUNTER GET)
              (4 ifOutMulticastPkts COUNTER GET)
              (5 ifOutBroadcastPkts COUNTER GET)
              (6 ifHCInOctets COUNTER64 GET)
              (7 ifHCInUcastPkts COUNTER64 GET)
              (8 ifHCInMulticastPkts COUNTER64 GET)
              (9 ifHCInBroadcastPkts COUNTER64 GET)
              (10 ifHCOutOctets COUNTER64 GET)
              (11 ifHCOutUcastPkts COUNTER64 GET)
              (12 ifHCOutMulticastPkts COUNTER64 GET)
              (13 ifHCOutBroadcastPkts COUNTER64 GET)
              (14 ifLinkUpDownTrapEnable INTEGER GET SET)
              (15 ifHighSpeed GAUGE GET)
              (16 ifPromiscuousMode INTEGER GET SET)
              (17 ifConnectorPresent INTEGER GET)
              (18 ifAlias OCTETSTRING GET)
              (19 ifCounterDiscontinuityTime TIMETICKS GET)
          ))
          (2 ifStackTable
            (1 ifStackEntry : INTEGER INTEGER op_ifstack
              (1 ifStackHigherLayer INTEGER)
              (2 ifStackLowerLayer INTEGER)
              (3 ifStackStatus INTEGER GET)
          ))
          (4 ifRcvAddressTable
            (1 ifRcvAddressEntry : INTEGER OCTETSTRING op_rcvaddr
              (1 ifRcvAddressAddress OCTETSTRING)
              (2 ifRcvAddressStatus INTEGER GET)
              (3 ifRcvAddressType INTEGER GET)
          ))
          (5 ifTableLastChange TIMETICKS op_ifmib GET)
          (6 ifStackLastChange TIMETICKS op_ifmib GET)
        )
      )
      (48 ipMIB
      )
      (49 tcpMIB
      )
      (50 udpMIB
      )
  ))
  (4 private
    (1 enterprises
      (12325 fokus
        (1 begemot
	  (3 begemotIp
	    (1 begemotIpObjects
	      (1 begemotMib2
		(1 begemotIfMaxspeed COUNTER64 op_begemot_mibII GET)
		(2 begemotIfPoll TIMETICKS op_begemot_mibII GET)
		(3 begemotIfForcePoll TIMETICKS op_begemot_mibII GET SET)
		(4 begemotIfDataPoll TIMETICKS op_begemot_mibII GET SET)
	      )
	    )
	  )
        )
      )
    )
  )
  (6 snmpV2
    (3 snmpModules
      (1 snmpMIB
        (1 snmpMIBObjects
          (5 snmpTraps
            (3 linkDown OID op_snmp_trap)
            (4 linkUp OID op_snmp_trap)
          )
        )
      )
  ))
)
